{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Energy Balance_20240424.xlsx"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Energy Balance_20240424.xlsx","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["","24 Apr 24 Daily peak [MW]","24 Apr 24 Daily energy [GWh]","Eq. day 23 Daily energy [GWh]","Apr 24 Accumulated energy [GWh]","Monthly variation [%]"]
["TOTAL GENERATION",9090,127,108,3480,60.1]
["Renewable Generation",8359,100,61,3051,93.3]
["Hydro 1",6465,48,14,1590,362.5]
["Wind",1945,26,32,909,23.5]
["Solar",2017,17,7,338,15.8]
["Wave",0,0,"",0,"-"]
["Biomass 2",403,9,8,215,3.8]
["Cogeneration",183,4,4,92,6.5]
["Others",223,5,4,124,1.9]
["Non-Renewable Generation",752,7,42,152,-57.7]
["Natural Gas",727,6,42,135,-61]
["Combined-Cycle",538,2,36,36,-84.9]
["Cogeneration",202,4,6,100,-10.5]
["Other Thermal 3",27,1,0,17,37.1]
["Cogeneration",4,0,0,2,44.7]
["Others",22,1,0,15,36.1]
["Generation from Storage","",20,5,276,17]
["Pumped Storage Generation","",20,5,276,17]
["Battery Injection","",0,"",0,"-"]
["CONSUMPTION FOR STORAGE",1997,13,10,338,14.3]
["Pumping",1997,13,10,338,14.3]
["Batteries",0,0,"",0,"-"]
["IMPORT BALANCE",4003,19,42,58,-95]
["Imports (Commercial Schedules)",4434,39,45,700,-45.7]
["Exports (Commercial Schedules)",2450,21,4,642,365.1]
["CONSUMPTION",6726,133,140,3200,5.6]
["(Corrected by Temperature)","",132,142,3211,3.8]
[""]