{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Energy Balance_20240731.xlsx"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Energy Balance_20240731.xlsx","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["","31 Jul 24 Daily peak [MW]","31 Jul 24 Daily energy [GWh]","Eq. day 23 Daily energy [GWh]","Jul 24 Accumulated energy [GWh]","Monthly variation [%]"]
["TOTAL GENERATION",6414,98,112,2996,-8.8]
["Renewable Generation",5498,66,91,2311,25.2]
["Hydro 1",3714,22,10,625,147.9]
["Wind",1637,14,60,770,-16.4]
["Solar",2501,20,13,651,49.6]
["Wave",0,0,"",0,"-"]
["Biomass 2",400,9,8,265,11.8]
["Cogeneration",185,4,3,118,31.4]
["Others",218,5,5,147,-0.1]
["Non-Renewable Generation",985,21,14,392,-67.8]
["Natural Gas",959,21,13,375,-68.5]
["Combined-Cycle",766,15,5,220,-77.9]
["Cogeneration",266,6,8,155,-21.1]
["Other Thermal 3",28,1,1,16,-24.7]
["Cogeneration",5,0,0,2,-37.1]
["Others",23,1,1,14,-22.8]
["Generation from Storage","",11,8,293,30.4]
["Pumped Storage Generation","",11,8,293,30.4]
["Battery Injection","",0,"",0,"-"]
["CONSUMPTION FOR STORAGE",1558,6,11,355,17.8]
["Pumping",1558,6,11,355,17.8]
["Batteries",0,0,"",0,"-"]
["IMPORT BALANCE",3690,57,44,1674,40.3]
["Imports (Commercial Schedules)",3801,59,48,1833,40.7]
["Exports (Commercial Schedules)",509,3,4,163,44.9]
["CONSUMPTION",7088,149,145,4315,3.3]
["(Corrected by Temperature)","",145,146,4295,3.1]
[""]