{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Energy Balance_20240917.xlsx"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Energy Balance_20240917.xlsx","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["","17 Sep 24 Daily peak [MW]","17 Sep 24 Daily energy [GWh]","Eq. day 23 Daily energy [GWh]","Sep 24 Accumulated energy [GWh]","Monthly variation [%]"]
["TOTAL GENERATION",6018,116,92,1764,-0.8]
["Renewable Generation",5580,95,37,1344,38.7]
["Hydro 1",3374,7,10,202,20.9]
["Wind",3624,62,7,680,33.6]
["Solar",2130,16,13,310,93]
["Wave",0,0,"",0,"-"]
["Biomass 2",398,9,7,153,15]
["Cogeneration",192,4,3,74,29]
["Others",210,5,5,79,4.6]
["Non-Renewable Generation",601,10,50,245,-62.9]
["Natural Gas",568,9,50,235,-64.1]
["Combined-Cycle",373,5,45,166,-71]
["Cogeneration",205,4,5,69,-16.3]
["Other Thermal 3",34,1,0,10,74.6]
["Cogeneration",5,0,0,2,-26.9]
["Others",29,1,0,8,134.2]
["Generation from Storage","",12,5,175,16.5]
["Pumped Storage Generation","",12,5,175,16.5]
["Battery Injection","",0,"",0,"-"]
["CONSUMPTION FOR STORAGE",1921,13,11,239,27.8]
["Pumping",1921,13,11,239,27.8]
["Batteries",0,0,"",0,"-"]
["IMPORT BALANCE",3404,43,55,771,16.4]
["Imports (Commercial Schedules)",4195,52,59,863,15.7]
["Exports (Commercial Schedules)",1026,9,4,94,11]
["CONSUMPTION",7516,146,136,2297,1.9]
["(Corrected by Temperature)","",142,136,2326,3.5]
[""]