{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Energy Balance_20250324.xlsx"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Energy Balance_20250324.xlsx","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["","24 Mar 25 Daily peak [MW]","24 Mar 25 Daily energy [GWh]","Eq. day 24 Daily energy [GWh]","Mar 25 Accumulated energy [GWh]","Monthly variation [%]"]
["TOTAL GENERATION",9701,171,194,3942,-8.6]
["Renewable Generation",8700,144,158,3333,-7.8]
["Hydro 1",6543,72,83,1584,-20.4]
["Wind",2679,44,56,1296,12.6]
["Solar",2480,20,9,277,7.8]
["Wave",0,0,0,0,"-"]
["Biomass 2",350,8,9,175,-19.7]
["Cogeneration",193,4,4,75,-23.9]
["Others",171,4,5,100,-16.2]
["Non-Renewable Generation",1108,13,12,360,-16.3]
["Natural Gas",1099,13,11,350,-15.3]
["Combined-Cycle",944,9,7,269,-15.2]
["Cogeneration",174,4,4,82,-15.9]
["Other Thermal 3",10,0,1,10,-40.5]
["Cogeneration",6,0,0,2,3]
["Others",4,0,1,7,-47.3]
["Generation from Storage","",14,24,249,-5.8]
["Pumped Storage Generation","",14,24,249,-5.8]
["Battery Injection","",0,0,0,-11.1]
["CONSUMPTION FOR STORAGE",1745,17,5,334,-11.3]
["Pumping",1745,17,5,334,-11.3]
["Batteries",0,0,0,0,29.8]
["IMPORT BALANCE",2128,3,-48,66,"+/-"]
["Imports (Commercial Schedules)",3223,29,4,536,38.8]
["Exports (Commercial Schedules)",3385,27,52,471,-40.8]
["CONSUMPTION",8649,157,141,3675,4.3]
["(Corrected by Temperature)","",151,147,3635,3.1]
[""]