{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Energy Balance_20250423.xlsx"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Energy Balance_20250423.xlsx","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["","23 Apr 25 Daily peak [MW]","23 Apr 25 Daily energy [GWh]","Eq. day 24 Daily energy [GWh]","Apr 25 Accumulated energy [GWh]","Monthly variation [%]"]
["TOTAL GENERATION",7956,136,127,3436,2.5]
["Renewable Generation",7265,109,100,2875,-2.6]
["Hydro 1",6467,68,48,1427,-7.4]
["Wind",1178,11,26,951,7.7]
["Solar",2475,23,17,317,-1.3]
["Wave",0,0,0,0,"-"]
["Biomass 2",313,7,9,181,-12.3]
["Cogeneration",163,4,4,91,4.3]
["Others",159,4,5,89,-24.6]
["Non-Renewable Generation",697,11,7,251,73.1]
["Natural Gas",672,10,6,241,86.8]
["Combined-Cycle",513,7,2,169,404.3]
["Cogeneration",164,3,4,72,-24.8]
["Other Thermal 3",26,1,1,10,-36.9]
["Cogeneration",3,0,0,1,-18.9]
["Others",23,0,1,9,-39.2]
["Generation from Storage","",16,20,310,21.1]
["Pumped Storage Generation","",16,20,310,21]
["Battery Injection","",0,0,0,">"]
["CONSUMPTION FOR STORAGE",2483,20,13,348,7]
["Pumping",2479,20,13,348,7]
["Batteries",4,0,0,0,">"]
["IMPORT BALANCE",3576,23,19,71,82.8]
["Imports (Commercial Schedules)",4358,47,39,602,-8.9]
["Exports (Commercial Schedules)",2193,24,21,532,-14.4]
["CONSUMPTION",7324,140,133,3160,3]
["(Corrected by Temperature)","",140,132,3204,4.1]
[""]