{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Energy Balance_20250427.xlsx"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Energy Balance_20250427.xlsx","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["","27 Apr 25 Daily peak [MW]","27 Apr 25 Daily energy [GWh]","Eq. day 24 Daily energy [GWh]","Apr 25 Accumulated energy [GWh]","Monthly variation [%]"]
["TOTAL GENERATION",8255,127,114,3992,1.3]
["Renewable Generation",7485,104,96,3342,-3.3]
["Hydro 1",6200,40,50,1646,-8.1]
["Wind",2381,34,21,1085,4.3]
["Solar",2409,21,16,400,5.4]
["Wave",0,0,0,0,"-"]
["Biomass 2",355,8,9,211,-13.6]
["Cogeneration",178,4,4,106,2]
["Others",179,4,5,105,-25.1]
["Non-Renewable Generation",839,12,4,292,78]
["Natural Gas",814,11,3,279,92.5]
["Combined-Cycle",698,8,0,195,448.3]
["Cogeneration",131,3,2,84,-23.4]
["Other Thermal 3",27,1,1,12,-33.9]
["Cogeneration",5,0,0,2,-15.7]
["Others",22,0,1,11,-36.4]
["Generation from Storage","",12,14,358,11.8]
["Pumped Storage Generation","",11,14,358,11.8]
["Battery Injection","",0,0,0,">"]
["CONSUMPTION FOR STORAGE",2501,21,25,439,15.2]
["Pumping",2498,21,25,438,15.2]
["Batteries",4,0,0,0,">"]
["IMPORT BALANCE",2321,3,23,90,">"]
["Imports (Commercial Schedules)",3444,33,41,735,-1.4]
["Exports (Commercial Schedules)",2534,30,18,647,-13]
["CONSUMPTION",5978,110,112,3644,2.3]
["(Corrected by Temperature)","",111,112,3692,3.2]
[""]