{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Energy Balance_20250509.xlsx"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Energy Balance_20250509.xlsx","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["","09 May 25 Daily peak [MW]","09 May 25 Daily energy [GWh]","Eq. day 24 Daily energy [GWh]","May 25 Accumulated energy [GWh]","Monthly variation [%]"]
["TOTAL GENERATION",7659,127,91,1278,20.3]
["Renewable Generation",6635,99,80,1029,15.8]
["Hydro 1",5842,65,44,537,83.2]
["Wind",748,8,8,262,-28.8]
["Solar",2082,18,19,163,13]
["Wave",0,0,0,0,"-"]
["Biomass 2",348,8,10,67,-19.9]
["Cogeneration",159,4,4,28,-23.6]
["Others",193,4,5,39,-17.1]
["Non-Renewable Generation",1127,24,4,177,346]
["Natural Gas",1103,23,3,171,420.5]
["Combined-Cycle",942,19,0,143,">"]
["Cogeneration",169,3,4,28,-11.5]
["Other Thermal 3",27,1,1,6,-13.7]
["Cogeneration",3,0,0,1,-24.2]
["Others",24,1,1,5,-12.2]
["Generation from Storage","",5,7,72,-46]
["Pumped Storage Generation","",5,7,72,-46]
["Battery Injection","",0,0,0,"-"]
["CONSUMPTION FOR STORAGE",948,6,9,71,-57.1]
["Pumping",948,6,9,71,-57.1]
["Batteries",0,0,0,0,43.2]
["IMPORT BALANCE",1015,16,54,-55,"-/+"]
["Imports (Commercial Schedules)",1230,20,65,48,-87.8]
["Exports (Commercial Schedules)",1299,4,11,103,12.2]
["CONSUMPTION",6771,137,136,1152,-3.6]
["(Corrected by Temperature)","",138,135,1160,-2.6]
[""]