{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Energy Balance_20260220.xlsx"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Energy Balance_20260220.xlsx","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["","20 Feb 26 Daily peak [MW]","20 Feb 26 Daily energy [GWh]","Eq. day 25 Daily energy [GWh]","Feb 26 Accumulated energy [GWh]","Monthly variation [%]"]
["TOTAL GENERATION",8472,170,160,3829,20.4]
["Renewable Generation",6945,128,137,2964,14.2]
["Hydro 1",5734,90,44,1307,-17.6]
["Wind",1018,12,81,1383,119.5]
["Solar",2609,19,5,140,-37.7]
["Wave",0,0,0,0,"-"]
["Biomass 2",277,6,7,134,-13.6]
["Cogeneration",91,2,3,59,-5]
["Others",190,4,5,75,-19.4]
["Non-Renewable Generation",2301,32,16,724,72.3]
["Natural Gas",2269,31,16,712,75.4]
["Combined-Cycle",2152,29,12,659,98]
["Cogeneration",127,3,4,53,-27.7]
["Other Thermal 3",34,1,1,12,-16.3]
["Cogeneration",5,0,0,2,5.1]
["Others",29,1,1,11,-18.8]
["Generation from Storage","",10,7,140,-13.7]
["Pumped Storage Generation","",10,7,140,-13.8]
["Battery Injection","",0,0,0,420.7]
["CONSUMPTION FOR STORAGE",1379,10,8,208,2.4]
["Pumping",1374,10,8,207,2.3]
["Batteries",12,0,0,0,633.2]
["IMPORT BALANCE",1394,8,14,-253,"-/+"]
["Imports (Commercial Schedules)",1500,16,25,114,-78.2]
["Exports (Commercial Schedules)",1506,8,12,368,15.3]
["CONSUMPTION",8776,168,166,3368,6.2]
["(Corrected by Temperature)","",171,174,3442,6.1]
[""]