{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Energy Balance_20260313.xlsx"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Energy Balance_20260313.xlsx","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["","13 Mar 26 Daily peak [MW]","13 Mar 26 Daily energy [GWh]","Eq. day 25 Daily energy [GWh]","Mar 26 Accumulated energy [GWh]","Monthly variation [%]"]
["TOTAL GENERATION",9244,152,182,2130,5.1]
["Renewable Generation",8373,121,145,1690,-1.5]
["Hydro 1",5280,58,73,973,21]
["Wind",3333,39,43,441,-35.6]
["Solar",2458,16,22,186,43.7]
["Wave",0,0,0,0,"-"]
["Biomass 2",314,7,7,90,-6.3]
["Cogeneration",90,2,3,26,-31.4]
["Others",229,5,4,64,10.3]
["Non-Renewable Generation",1032,21,22,314,55.6]
["Natural Gas",999,20,22,305,55.9]
["Combined-Cycle",923,18,17,281,82.4]
["Cogeneration",79,2,5,24,-42]
["Other Thermal 3",34,1,0,9,49]
["Cogeneration",5,0,0,1,15.5]
["Others",29,1,0,8,54.3]
["Generation from Storage","",11,14,126,14.6]
["Pumped Storage Generation","",11,14,125,14.1]
["Battery Injection","",0,0,1,">"]
["CONSUMPTION FOR STORAGE",2015,17,21,146,-4.4]
["Pumping",2014,17,21,145,-4.8]
["Batteries",15,0,0,1,">"]
["IMPORT BALANCE",3522,30,-4,69,-44.7]
["Imports (Commercial Schedules)",3500,36,17,245,-22.5]
["Exports (Commercial Schedules)",1296,6,21,178,-8]
["CONSUMPTION",8573,166,157,2054,2.8]
["(Corrected by Temperature)","",163,154,2046,2.5]
[""]