{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Energy Balance_20260405.xlsx"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Energy Balance_20260405.xlsx","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["","05 Apr 26 Daily peak [MW]","05 Apr 26 Daily energy [GWh]","Eq. day 25 Daily energy [GWh]","Apr 26 Accumulated energy [GWh]","Monthly variation [%]"]
["TOTAL GENERATION",6420,94,153,575,-29.6]
["Renewable Generation",5605,56,132,378,-44.5]
["Hydro 1",4932,26,55,134,-58.6]
["Wind",638,7,58,114,-56]
["Solar",2090,15,12,91,48.4]
["Wave",0,0,0,0,"-"]
["Biomass 2",360,8,8,40,1.7]
["Cogeneration",143,3,4,16,-16.3]
["Others",219,5,4,24,19.6]
["Non-Renewable Generation",996,20,9,99,74.1]
["Natural Gas",967,19,8,95,72.7]
["Combined-Cycle",911,18,6,88,130.3]
["Cogeneration",58,1,2,8,-55.7]
["Other Thermal 3",31,1,1,4,119.2]
["Cogeneration",3,0,0,0,2.2]
["Others",29,1,0,3,145.1]
["Generation from Storage","",18,12,98,24.2]
["Pumped Storage Generation","",18,12,98,24]
["Battery Injection","",0,0,0,">"]
["CONSUMPTION FOR STORAGE",2736,22,11,105,59.7]
["Pumping",2725,22,11,105,59.3]
["Batteries",15,0,0,0,">"]
["IMPORT BALANCE",3670,31,-29,152,"+/-"]
["Imports (Commercial Schedules)",3729,37,14,190,93.9]
["Exports (Commercial Schedules)",1114,7,42,38,-70.9]
["CONSUMPTION",5433,103,113,623,-13.2]
["(Corrected by Temperature)","",106,113,642,-12.8]
[""]