{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Balanço Energético_20231210.xls"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Balanço Energético_20231210.xls","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
["","10 dez 23 Ponta diária [MW]","10 dez 23 Energia diária [GWh]","Dia eq. 22 Energia diária [GWh]","dez 23 Energia acumulada [GWh]","Variação mensal [%]"]
["PRODUÇÃO TOTAL",7733,117,167,1540,0.7]
["Produção Renovável",7561,105,117,1236,35.4]
["Hídrica 1",5426,52,49,665,40.7]
["Eólica",2017,41,57,448,38]
["Solar",743,5,3,45,34.1]
["Ondas",0,0,"",0,"-"]
["Biomassa 2",335,8,8,78,-4.7]
["Cogeração",147,3,4,34,-2.6]
["Outros",192,4,5,44,-6.3]
["Produção não Renovável",182,4,45,214,-62.8]
["Gás Natural",169,4,45,210,-63]
["Ciclo Combinado",0,0,37,162,-66.6]
["Cogeração",177,4,8,48,-41.5]
["Outra Térmica 3",13,0,1,3,-48.9]
["Cogeração",4,0,0,1,65.6]
["Outros",9,0,1,2,-60.9]
["Produção por Armazenamento","",8,5,90,113.8]
["Produção por Bombagem","",8,5,90,113.8]
["CONSUMO PARA ARMAZENAMENTO",1836,13,7,112,54.9]
["Bombagem",1836,13,7,112,54.9]
["SALDO IMPORTADOR",2973,28,-28,76,"+/-"]
["Importação (valor comercial)",3075,33,2,235,69.4]
["Exportação (valor comercial)",1001,5,30,158,14.3]
["CONSUMO",6975,132,132,1504,3.2]
["(Corrigido da temperatura)","",139,135,1524,3.8]
["O uso desta informação implica a aceitação das condições de utilização."]