{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Energy Balance_20230930.xlsx"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Energy Balance_20230930.xlsx","index":0,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
["","Peak [MW]","Sep 23 [GWh]","Accumulated [GWh]","Sep 22 [GWh]","Accumulated [GWh]","Month [Variation %]","Accumulated [Variation %]"]
["TOTAL GENERATION",8117,3003,31317,3388,31186,-11.4,0.4]
["Renewable Generation",6933,1670,20983,1768,16864,-5.5,24.4]
["Hydro 1",5097,392,6782,343,3354,14,102.2]
["Wind",4341,726,9025,920,8872,-21,1.7]
["Solar",1798,318,2963,245,2083,29.9,42.2]
["Biomass 2",358,234,2213,259,2556,-10,-13.4]
["Cogeneration",162,94,885,101,1157,-7.3,-23.5]
["Others",218,139,1328,158,1399,-11.7,-5.1]
["Non-Renewable Generation",2794,1061,8234,1437,12715,-26.1,-35.2]
["Natural Gas",2778,1051,8070,1420,12571,-26,-35.8]
["Combined-Cycle",2548,906,6574,1239,10740,-26.9,-38.8]
["Cogeneration",289,145,1495,181,1832,-20,-18.4]
["Other Thermal 3",16,10,164,17,144,-40,14.1]
["Cogeneration",7,4,24,3,21,44.8,15.2]
["Others",10,6,140,14,123,-55.3,13.9]
["Generation from Storage","",272,2101,183,1606,48.2,30.8]
["Pumped Storage Generation","",272,2101,183,1606,48.2,30.8]
["CONSUMPTION FOR STORAGE",2474,322,2690,258,2072,24.8,29.8]
["Pumping",2474,322,2690,258,2072,24.8,29.8]
["IMPORT BALANCE",4361,1298,8850,862,8556,50.6,3.4]
["Imports (commercial schedules)",4495,1437,10878,1027,10128,39.9,7.4]
["Exports (commercial schedules)",2509,142,2044,164,1575,-13.6,29.8]
["CONSUMPTION",7222,3979,37478,3992,37669,-0.3,-0.5]
[""]