{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Energy Balance_20250331.xlsx"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Energy Balance_20250331.xlsx","index":0,"n_rows":28,"n_cols":8,"rows_kept":28,"cut":false,"hidden":false,"merged":[]}
["","Peak [MW]","Mar 25 [GWh]","Accumulated [GWh]","Mar 24 [GWh]","Accumulated [GWh]","Month [Variation %]","Accumulated [Variation %]"]
["TOTAL GENERATION",10942,4965,14113,5508,15050,-9.8,-6.2]
["Renewable Generation",10487,4180,11545,4672,12485,-10.5,-7.5]
["Hydro 1",6847,2035,5630,2484,6564,-18.1,-14.2]
["Wind",5078,1508,4205,1586,4331,-4.9,-2.9]
["Solar",2789,405,1016,320,782,26.6,29.9]
["Wave",0,0,0,0,0,"-","-"]
["Biomass 2",376,233,694,282,808,-17.4,-14.1]
["Cogeneration",194,105,284,128,345,-18.1,-17.8]
["Others",216,128,411,154,463,-16.9,-11.3]
["Non-Renewable Generation",1734,444,1720,475,1607,-6.5,7.1]
["Natural Gas",1719,433,1668,454,1543,-4.6,8.1]
["Combined-Cycle",1547,327,1349,331,1130,-1.3,19.4]
["Cogeneration",215,106,319,122,413,-13.6,-22.6]
["Other Thermal 3",31,11,52,21,64,-47.9,-18.8]
["Cogeneration",5,2,7,3,9,-15.4,-25.9]
["Others",28,9,46,18,55,-52.9,-17.7]
["Generation from Storage","",341,847,361,958,-5.6,-11.6]
["Pumped Storage Generation","",341,847,361,958,-5.6,-11.6]
["Battery Injection","",0,0,0,0,5.8,-31.8]
["CONSUMPTION FOR STORAGE",2593,471,1116,477,1191,-1.2,-6.3]
["Pumping",2593,471,1116,477,1191,-1.2,-6.3]
["Batteries",1,0,0,0,0,29.5,69.2]
["IMPORT BALANCE",4711,156,1070,-507,-160,"+/-","+/-"]
["Imports (commercial schedules)",4768,784,2606,476,1874,64.5,39.1]
["Exports (commercial schedules)",3641,630,1534,983,2034,-35.9,-24.6]
["CONSUMPTION",8988,4651,14067,4524,13700,2.8,2.7]
[""]