{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Energy Balance_20250430.xlsx"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Energy Balance_20250430.xlsx","index":0,"n_rows":28,"n_cols":8,"rows_kept":28,"cut":false,"hidden":false,"merged":[]}
["","Peak [MW]","Apr 25 [GWh]","Accumulated [GWh]","Apr 24 [GWh]","Accumulated [GWh]","Month [Variation %]","Accumulated [Variation %]"]
["TOTAL GENERATION",10547,4367,18498,4343,19393,0.6,-4.6]
["Renewable Generation",10131,3636,15200,3804,16289,-4.4,-6.7]
["Hydro 1",6634,1794,7425,1965,8529,-8.7,-12.9]
["Wind",4813,1187,5407,1143,5474,3.9,-1.2]
["Solar",2701,425,1446,423,1205,0.5,20]
["Wave",0,0,0,0,0,"-","-"]
["Biomass 2",375,229,922,273,1081,-16,-14.7]
["Cogeneration",196,115,398,116,461,-0.9,-13.7]
["Others",194,114,524,156,620,-27.2,-15.4]
["Non-Renewable Generation",1843,346,2066,179,1786,93.1,15.7]
["Natural Gas",1824,332,2000,158,1701,110.2,17.6]
["Combined-Cycle",1707,243,1592,38,1168,536.2,36.2]
["Cogeneration",184,89,409,120,532,-25.5,-23.3]
["Other Thermal 3",27,14,66,21,86,-34.9,-22.8]
["Cogeneration",6,2,9,3,11,-16.6,-24.1]
["Others",23,12,57,19,74,-37.4,-22.6]
["Generation from Storage","",385,1232,360,1318,7,-6.5]
["Pumped Storage Generation","",385,1232,360,1318,7,-6.5]
["Battery Injection","",0,0,0,0,">",">"]
["CONSUMPTION FOR STORAGE",2702,460,1575,423,1614,8.6,-2.4]
["Pumping",2698,459,1575,423,1614,8.6,-2.4]
["Batteries",5,0,0,0,0,">",">"]
["IMPORT BALANCE",4206,82,1152,27,-133,207.6,"+/-"]
["Imports (commercial schedules)",4405,803,3409,830,2704,-3.2,26.1]
["Exports (commercial schedules)",4226,704,2238,804,2838,-12.4,-21.1]
["CONSUMPTION",7709,3989,18075,3946,17646,1.1,2.4]
[""]