{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["caracterização da rnt_20241231."],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"caracterização da rnt_20241231.","index":0,"n_rows":14,"n_cols":2,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["",2024]
["Comprimento das Linhas [km]",9661]
["400 kV",3242]
["220 kV",3886]
["150 kV",2533]
["Potência de Transformação [MVA]",40729]
["Autotransformação (MAT/MAT)",15370]
["Transformação (MAT/AT)",25039]
["Transformação (MAT/MT)",320]
["Subestações",71]
["Postos de Corte",14]
["Postos de Seccionamento",2]
["Postos de Transição",1]
[""]